**4-Cyl Paint to Pass Rules**

**4 cyl. race cars are legal to run this race. Your roll cages do not need to be removed to participate. Newly built or used demo type 4 cyl. or V/6 cars can run. A legal V/6 car is one that was also offered with a 4 cyl. Engine the rules below are for the demo type cars. The 4 cyl. racing cars should meet all safety requirements. Your door bars and cage should also meet the roll over poll and door bar rules.**

Remove **all glass**, fiberglass, headlights, tail lights, trim, interior, trailer hitches, etc. Cars must be swept clean. No junk tires, wheels, metal parts, etc. allowed.   
Must have screen or windshield in place with two protection bars in front of driver.

Side window net required

All rear seats and floor decking must be removed. Any sharp or protruding fins must be cut off the vehicle.   
  
5 point racing harness required, approved helmet, and eye protection (face shield or safety glasses) are required. Neck braces are highly recommended. Fire retardant suits, clothing, and head sock are recommended.   
  
Drivers MUST wear long sleeved shirts and long pants during their heat. NO shorts allowed!!   
  
All hoods must have a 6x6 square holes on each side [one on each side] of hood so safety can put out a fire   
  
All vehicles must have dependable brakes at all times.   
  
Stock gas tanks may be used if forward of rear axle. A replacement tank must be securely fastened in the rear section (no farther forward than the back of the front seat) of the driver’s compartment. Steel gas tanks or Neoprene construction approved tanks may be used. Gas tank must be securely fastened by means other than ratchet straps or wire. Tanks must be securely bolted to the floor. Tanks must be covered in a fireproof fashion. Any vehicle that spills gas will be disqualified immediately.   
  
Electric fuel pumps are permitted.  
  
Stock batteries must be removed from the original position. A battery must be located in the driver’s compartment and securely fastened to the floor. The battery must also be covered.   
  
No profanity will be permitted on any vehicle  
  
Doors must be fastened shut by chain, or welding. No loose doors permitted.   
Use enough chain to securely and safely fasten the door. No chaining to the frame.  
  
A protection bar must be used on the driver’s door. A grader bar or channel bar [6 inch is a good size] with 4 1/2 inch or larger bolts over the original driver’s door skin. and be within the boundaries of below the window and above your hips bar must be forward of door edge and far enough back to go past the B pillar.  
  
A roll over poll must be used. Placed behind driver from floor to roof min. 3 inch material round or square. A min. 10" square plate welded to top and bottom and bolted to roof and floor with 4 1/2 inch bolts top and bottom. a spreader bar must be used between B pillars behind [ recommended to tie this to roll over poll ]

call with questions   Jody turner 503-369-0127